REMOVAL ■ CAUTION ■ Disconnect the battery negative terminal or the remove the fuse.

1.Remove the rear wing. Refer to Exploded View.

2.Remove the center leg bracket.

3.Remove the high-mounted stop lamp mounting screw. And then cut the two-sided tape by the any appropriate tool (A).

4.Disconnect the connector. And then remove the high-mounted stop lamp from the rear wing.

INSTALLATION
Install in the reverse order of removal.