1.CHECK POWER DOOR LOCK OPERATION Check power door lock operation. Does door lock/unlock with door lock and unlock switch? YES>>GO TO 2. NO>>Refer to Diagnosis Procedure.
2.CHECK REMOTE KEYLESS ENTRY RECEIVER
Check remote keyless entry receiver.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CHECK INTELLIGENT KEY
Check Intelligent Key.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 4.
NO>>Repair or replace the malfunctioning parts.
4.CHECK KEY SLOT
Check key slot.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 5.
NO>>Repair or replace the malfunctioning parts.
5.CHECK DOOR SWITCH
Check door switch.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 6.
NO>>Repair or replace the malfunctioning parts.
6.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.