DESCRIPTION In FOOT mode, the air blowing to DEF can change ON/OFF. HOW TO SET With CONSULT-III Perform the “BLOW SET” of HVAC work support item.

Work support items | Display | Defroster door position
Auto control | Manual control
BLOW SET | MODE 1 | OPEN | CLOSE
MODE 2 (initial status) | OPEN | OPEN
MODE 3 | CLOSE | OPEN
MODE 4 | CLOSE | CLOSE

NOTE：
When the battery cable is disconnected from the negative terminal or when the battery voltage becomes 10 V or less, the setting of the discharge air mix ratio in FOOT mode may be cancelled.