■ CAUTION ■ When removing, always use a remover tool that is made of plastic. REMOVAL

1.Remove the rear console assembly.

- Lift up the rear side of rear console assembly (1), and then disengage the pawls and the metal clips.
- Disconnect the harness connector on the back.

  | : Pawl
  | : Metal clip

2.Remove the instrument garnish LH.

- Insert the remover tool (A), wrapped in a shop cloth, into the clearance between the lower side of instrument garnish LH (1) and the cluster lid C (lower) (2).
- Pull back the instrument garnish LH, and then disengage the pawls.

  | : Pawl

3.Remove the instrument garnish RH.

- Insert the remover tool (A), wrapped in a shop cloth, into the clearance between the lower side of instrument garnish RH (1) and the cluster lid C (lower) (2).
- Pull back the instrument garnish RH, and then disengage the pawls.

  | : Pawl

4.Remove the console finisher.

- Open the console lid.
- Insert the remover tool (A) between the console finisher (1) and the center console, lift up the console finisher, and then disengage the clips and the pawls.

  | : Clip
  | : Pawl

5.Remove the instrument side panel LH. Pull the instrument side panel LH (1) from vehicle front in lateral direction, then disengage the clips, pawl and the metal clips.
■ CAUTION ■
Be careful of the pawl when disengaging the clips.

| : Clip
| : Pawl
| : Metal clip

6.Remove the instrument side panel RH. Pull the instrument side panel RH (1) from vehicle front in lateral direction, then disengage the clips, pawl and the metal clips.
■ CAUTION ■
Be careful of the pawl when disengaging the clips.

| : Clip
| : Pawl
| : Metal clip

7.Remove the center console assembly.

- Remove the mounting screws (A) from front end of the center console (1).
- Remove the mounting nuts (B) from rear end of the center console.
- Lift up the center console, and then remove the harness clamps (C) and disconnect the harness connector from back side.

INSTALLATION
Install in the reverse order of removal.