Items | Transmission unit harness connector | Resistance (Approx.)
Connector | Terminal
Transmission oil temperature 20°C (68°F) | Transmission oil temperature 50°C (122°F) | Transmission oil temperature 80°C (176°F)
Shift solenoid valve 1 | B49 | 13 | Ground | 6.6–7.4Ω | 7.3–8.3Ω | 8.1–9.2Ω
Shift solenoid valve 2 | 20
Shift solenoid valve 3 | 27
Shift solenoid valve 4 | 7
Sequence solenoid valve | 6
Axis A feed pressure solenoid valve | 14 | 15 | 3.8–4.4Ω | 4.3–5.0Ω | 4.7–5.4Ω
Axis B feed pressure solenoid valve | 21 | 22
Clutch A solenoid valve | B50 | 37 | 38 | 4.6–5.0Ω | 5.1–5.6Ω | 5.6–6.2Ω
Clutch B solenoid valve | 42 | 43
Line pressure solenoid valve | 48 | 49 | 3.8–4.4Ω | 4.3–5.0Ω | 4.7–5.4Ω
Lubricating flow solenoid valve | 54 | 55