Checks the entire SRS and displays the malfunction either by illuminating or blinking the air bag warning lamp on the combination meter. Malfunctioning part can be detected by on board self-diagnosis system and CONSULT-III. OPERATION It detects a shock that exceeds a specified level and monitors whether the driver and passenger air bags, front side air bag, side curtain air bag, and pre-tensioner seat belts operate normally.
STRUCTURE
It contains the “G” sensors for both frontal and side collisions and spare battery function in case of main battery damage in collision.
INSTALLATION
Air bag diagnosis sensor unit is installed under the center console with fixed bolts.