INSPECTION

1.Remove tires. Refer to Exploded View.

2.Check the thickness of brake pad from the inspection hole on caliper. Use a scale to check if necessary.

Wear thickness | : Refer to Front Disc Brake.

3.Check the brake pad for whitening (carbonizing) and uneven wear. Replace if necessary. Refer to Exploded View (GT-R certified NISSAN dealer).
■ CAUTION ■
Replace the brake pad and disc rotor of all wheels as a set. [However, the brake pads can be separately replaced onlywhen a certified technician checks for scratches and cracksand judges that the brake disc rotors are reusable. (For the disc rotor, two sets of brake pad at amaximum.) Refer to Inspection and Adjustment and Inspection (GT-R certified NISSAN dealer).

4.Install tires. Refer to Exploded View.

ADJUSTMENT
Perform the following procedure when replacing the brake pad and disc rotor.
■ CAUTION ■

- Be careful of the vehicle speed, because the effectiveness of the brake is decreased by the anti-corrosion paint (silver color) applied for the contact surface with the brake pad for new disc rotor.
- Perform the procedure only on a safe road and be careful of the traffic conditions.

1.Drive on flat straight roads.

2.Depress the brake pedal to stop the vehicle within 3 to 5 seconds.

3.Cool the brake.

4.Repeat the above steps 1 to 3 until the operational feeling of brake pedal becomes equal to the pre-operation condition.

5.Check that the anti-corrosion paint (silver color) of disc rotor is eliminated. If the anti-corrosion paint (silver color) remains, repeat the above steps 1 to 3.

6.If brake noise occurs, loosen the caliper mounting bolts after checking that the anti-corrosion paint (silver color) does not remain at the disc rotor, and then perform the caliper position adjustment by tightening to the specified torque. Refer to Removal and Installation (GT-R certified NISSAN dealer).
■ CAUTION ■
If the anti-corrosion paint (silver color) remains on the surface of brake pad, polish it with sandpaper until completely eliminated.

7.Use a brake tester to check that it is within the normal range.