The actual shapes of Kent-Moore tools may differ from those of special service tools illustrated here.
Tool number (Kent-Moore No.) Tool name | Description
KV381054S0 (J-34286) Puller |  |

- Removing side oil seal (right side)
- Removing side bearing outer race

ST33400001 (J-26082) Drift a: 60 mm (2.36 in) dia. b: 47 mm (1.85 in) dia.

- Installing side oil seal (right side)
- Installing front oil seal

KV38102100 (J-25803-01) Drift a: 44 mm (1.73 in) dia. b: 36 mm (1.42 in) dia.
c: 24.5 mm (0.965 in) dia.
Installing side oil seal (left side)
KV38100200 (　　—　　) Drift a: 65 mm (2.56 in) dia. b: 49 mm (1.93 in) dia.
Installing side shaft oil seal
ST30032000 (J-26010-01) Drift a: 80 mm (3.15 in) dia. b: 38 mm (1.50 in) dia.
c: 31 mm (1.22 in) dia.

- Installing side shaft
- Installing pinion rear bearing inner race

ST3306S001 (J-22888-D) Differential side bearing puller set 1: ST33051001 (J-22888-20)
Puller
2: ST33061000
(J-8107-2)
Base
a: 28.5 mm (1.122 in) dia.
b: 38 mm (1.50 in) dia.
Removing and installing side bearing inner race
ST33230000 (J-25805-01) Drift a: 51 mm (2.01 in) dia. b: 41 mm (1.61 in) dia.
c: 28.5 mm (1.122 in) dia.
Installing side bearing inner race
ST30611000 (J-25742-1) Drift bar |  | Installing side bearing outer race (Use with KV31103000)
KV31103000 (J-38982) Drift a: 49 mm (1.93 in) dia. b: 70 mm (2.76 in) dia.
Installing side bearing outer race
ST3127S000 (J-25765-A) Preload gauge |  | Measuring pinion bearing preload and total preload
(J-8129) Spring gauge |  | Measuring turning torque
ST37820000 (　　—　　) Drift a: 39 mm (1.54 in) dia. b: 72 mm (2.83 in) dia.
Installing pinion front and rear bearing outer race
KV38102510 (　　—　　) Drift a: 71 mm (2.80 in) dia. b: 65 mm (2.56 in) dia.
Installing front oil seal