1.CHECK A/T SHIFT SELECTOR (DETENTION SWITCH)

1. Turn ignition switch OFF.
2. Disconnect A/T shift selector connector.
3. Check continuity between A/T shift selector (detention switch) terminals.

   A/T shift selector (detention switch) | Condition | Continuity
   Terminal
   1 | 2 | Shift lever | P position | Not existed
   Other than above | Existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace A/T shift selector. Refer to Removal and Installation.