DTC DETECTION LOGIC

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B2014 | CHAIN OF S/L-BCM | Inactive communication between steering lock unit and BCM |

- Harness or connectors
  (Steering lock unit circuit is open or shorted)
- Steering lock unit
- BCM

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Lock steering.
2. Press the push-button ignition switch.
3. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END