Item | Function
BCM | Controls the door lock function and trunk open function.
IPDM E/R | Sounds horn and blinks head lamp via CAN communication between BCM.
Door lock actuator | Inputs lock/unlock signal from BCM and locks/unlocks each door.
Door switch | Inputs door open/close condition to BCM.
Key slot | Inputs key insert/remove signal to BCM.
Remote keyless entry receiver | Receives lock/unlock signal from the Intelligent Key, and then transmits to BCM.
Combination meter |

- Hazard warning lamp is installed to combination meter.
- Transmits vehicle seep signal to CAN communication line.

Intelligent Key | Transmits button operation to remote keyless entry receiver.
Trunk lid opener actuator | Transmits trunk lid open operation to BCM.
Trunk lid opener cancel switch | Cancels the trunk open operation.
Fuel lid lock actuator | Performs lock/unlock of the fuel lid.
Push-button ignition switch | Input push-button ignition switch ON/OFF condition to BCM.
Intelligent Key warning buzzer | Warns the user of the lock/unlock condition and inappropriate operations with the buzzer sound.
Hazard warning lamp | Warns the user of the door lock/unlock condition and in appropriate operations with the lamps blink.