1.CHECK TRUNK ROOM LAMP SWITCH

1. Turn ignition switch OFF.
2. Disconnect trunk lid lock assembly connector.
3. Check continuity between trunk lid lock assembly terminals.

   Terminal | Condition | Continuity
   Trunk lid lock assembly
   1 | 2 | Trunk lid | Open | Existed
   Closed | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace trunk lid lock assembly. Refer to Removal and Installation.