(Kent-Moore No.) Tool name |  | Description
(　—　) Power tool |  | Loosening nuts and bolts
(　—　) Manual lift table caddy |  | Removing and installing engine
(　—　) 1. Compression gauge 2. Adapter |  | Checking compression pressure
(　—　) Spark plug wrench |  | Removing and installing spark plug a: 14 mm (0.55 in)
(　—　) Valve seat cutter set |  | Finishing valve seat dimensions
(　—　) Piston ring expander |  | Removing and installing piston ring
(　—　) Valve guide drift |  | Removing and installing valve guide Intake and Exhaust: a: 9.5 mm (0.374 in) dia. b: 5.5 mm (0.217 in) dia.
(　—　) Valve guide reamer |  | A: Reaming valve guide inner hole B: Reaming hole for oversize valve guide Intake and Exhaust: c: 6.0 mm (0.236 in) dia. d: 10.2 mm (0.402 in) dia.
(J-43897-18) (J-43897-12) Oxygen sensor thread cleaner |  | Reconditioning the exhaust system threads before installing a new air fuel ratio sensor and heated oxygen sensor (Use with anti-seize lubricant shown below.) A: J-43897-18 [18 mm (0.71 in) dia.] for zirconia heated oxygen sensor and air fuel ratio sensor
B: J-43897-12 [12 mm (0.47 in) dia.] for titania heated oxygen sensor
C: Mating surface shave cylinder
D: Flutes
(　—　) Anti-seize lubricant (Permatex 133AR or equivalent meeting MIL specification MIL-A-907) |  | Lubricating oxygen sensor thread cleaning tool when reconditioning exhaust system threads