- The 6th-Neutral position sensor is installed on the actuator control valve and detects the sleeve A1 position.
- The 6th-Neutral position sensor converts the sleeve A1 position into output voltage and transmits the signal to TCM.
- The sleeve A1 has its oil passage secured by the shift solenoid valve 1 and shift solenoid valve 2 when the sequence solenoid valve is ON and is driven by the axis A feed pressure solenoid valve. The 6th gear is selected or deselected depending on the operation of the sleeve A1.