APPLICATION ITEM CONSULT-III performs the following functions via CAN communication with BCM.

Diagnosis mode | Function Description
Work Support | Changes the setting for each system function.
Self Diagnostic Result | Displays the diagnosis results judged by BCM.
CAN Diag Support Monitor | Monitors the reception status of CAN communication viewed from BCM. Refer to CONSULT-III operation manual.
Data Monitor | The BCM input/output signals are displayed.
Active Test | The signals used to activate each device are forcibly supplied from BCM.
Ecu Identification | The BCM part number is displayed.
Configuration | This function is not used even though it is displayed.

SYSTEM APPLICATION
BCM can perform the following functions for each system.
NOTE：
It can perform the diagnosis modes except the following for all sub system selection items.

×: Applicable item
System | Sub system selection item | Diagnosis mode
Work Support | Data Monitor | Active Test
Door lock | DOOR LOCK | × | × | ×
Rear window defogger | REAR DEFOGGER |  | × | ×
Warning chime | BUZZER |  | × | ×
Interior room lamp timer | INT LAMP | × | × | ×
Exterior lamp | HEAD LAMP | × | × | ×
Wiper and washer | WIPER | × | × | ×
Turn signal and hazard warning lamps | FLASHER | × | × | ×
— | AIR CONDITONER* |  | × |
Intelligent Key system | INTELLIGENT KEY | × | × | ×
Combination switch | COMB SW |  | × |
Body control system | BCM | × |  |
IVIS - NATS | IMMU |  | × | ×
Interior room lamp battery saver | BATTERY SAVER | × | × | ×
Trunk open | TRUNK |  | × |
Vehicle security system | THEFT ALM | × | × | ×
RAP system | RETAINED PWR |  | × |
Signal buffer system | SIGNAL BUFFER |  | × | ×
TPMS | TPMS (AIR PRESSURE MONITOR) | × | × | ×
*: This item is displayed, but is not used.

FREEZE FRAME DATA (FFD) AND IGN COUNTER
Freeze Frame Data
The BCM records the following condition at the moment a particular DTC is detected.

- Vehicle Speed
- Odo/Trip Meter
- Vehicle Condition (BCM detected condition)

  CONSULT screen terms | Description
  SLEEP>LOCK | While turning BCM status from low power consumption mode to normal mode (Power supply position is “LOCK”)
  SLEEP>OFF | While turning BCM status from low power consumption mode to normal mode (Power supply position is “OFF”.)
  LOCK>ACC | While turning power supply position from “LOCK” to “ACC”
  ACC>ON | While turning power supply position from “ACC” to “IGN”
  RUN>ACC | While turning power supply position from “RUN” to “ACC” (Vehicle is stopping and selector lever is except P position.)
  CRANK>RUN | While turning power supply position from “CRANKING” to “RUN” (From cranking up the engine to run it)
  RUN>URGENT | While turning power supply position from “RUN“ to “ACC” (Emergency stop operation)
  ACC>OFF | While turning power supply position from “ACC” to “OFF”
  OFF>LOCK | While turning power supply position from “OFF” to “LOCK”
  OFF>ACC | While turning power supply position from “OFF” to “ACC”
  ON>CRANK | While turning power supply position from “IGN” to “CRANKING”
  OFF>SLEEP | While turning BCM status from normal mode (Power supply position is “OFF”.) to low power consumption mode
  LOCK>SLEEP | While turning BCM status from normal mode (Power supply position is “LOCK”.) to low power consumption mode
  LOCK | Power supply position is “LOCK” (Ignition switch OFF with steering is locked.)
  OFF | Power supply position is “OFF” (Ignition switch OFF with steering is unlocked.)
  ACC | Power supply position is “ACC” (Ignition switch ACC)
  ON | Power supply position is “IGN” (Ignition switch ON with engine stopped)
  ENGINE RUN | Power supply position is “RUN” (Ignition switch ON with engine running)
  CRANKING | Power supply position is “CRANKING” (At engine cranking)

IGN Counter
IGN counter indicates the number of times that ignition switch is turned ON after DTC is detected.

- The number is 0 when a malfunction is detected now.
- The number increases like 1 → 2 → 3...38 → 39 after returning to the normal condition whenever ignition switch OFF → ON.
- The number is fixed to 39 until the self-diagnosis results are erased if it is over 39.