REMOVAL

1.Remove liquid tank. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Fix the liquid tank (1) with a vise (A). Remove the refrigerant pressure sensor (2) with a wrench (B).
■ CAUTION ■
Be careful not to damage liquid tank.

INSTALLATION
Installation is basically the reverse order of removal.
■ CAUTION ■

- Replace O-ring with new one. Then apply compressor oil to them when installing.
- Check for leakages when recharging refrigerant.