INSPECTION AFTER REMOVAL Use the standard type spark plug for normal condition.

Spark plug (Standard type) | : Refer to Spark Plug.

■ CAUTION ■

- Never drop or shock spark plug.
- Never use a wire brush for cleaning.
- If plug tip is covered with carbon, spark plug cleaner may be used.

  Cleaner air pressure:
  | Less than 588 kPa (6 kg/cm2, 85 psi)
  Cleaning time:
  | Less than 20 seconds

- Measure spark plug gap. When it exceeds the limit, replace spark plug even if it is within the specified replacement mileage. Refer to Spark Plug.
- Spark plug gap adjustment is not required between replacement intervals.