INSPECTION AFTER REMOVAL Check rear suspension member for deformation, cracks and damage. Replace if necessary. INSPECTION AFTER INSTALLATION

1.Check wheel sensor harness connector for proper connection. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Adjust parking brake operation (stroke). Inspection and Adjustment.

3.Check wheel alignment. Refer to Inspection.

4.Adjust neutral position of steering angle sensor. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).