WHEN NEW CYLINDER BLOCK AND CRANKSHAFT ARE USED

1.“MAIN BEARING SELECTION TABLE” rows correspond to bearing housing grade on rear left side of cylinder block.

A | : Cylinder bore grade No. 1
B | : Cylinder bore grade No. 2
C | : Cylinder bore grade No. 3
D | : Cylinder bore grade No. 4
E | : Cylinder bore grade No. 5
F | : Cylinder bore grade No. 6
G | : Bearing housing grade No. 1
H | : Bearing housing grade No. 2
I | : Bearing housing grade No. 3
J | : Bearing housing grade No. 4
| : Engine front

2.“MAIN BEARING SELECTION TABLE” columns correspond to journal diameter grade on front side of crankshaft.

A | : Journal diameter grade No. 1
B | : Journal diameter grade No. 2
C | : Journal diameter grade No. 3
D | : Journal diameter grade No. 4
E | : Pin diameter grade No. 1
F | : Pin diameter grade No. 2
G | : Pin diameter grade No. 3
H | : Pin diameter grade No. 4
I | : Pin diameter grade No. 5
J | : Pin diameter grade No. 6
K | : Identification code

3.Select main bearing grade at the point where selected row and column meet in “MAIN BEARING SELECTION TABLE”.

4.Apply the symbol obtained to the “MAIN BEARING GRADE TABLE” to select main bearing.
NOTE：

- “MAIN BEARING GRADE TABLE” applies to all journals.
- Service parts is available as a set of both upper and lower.

WHEN CYLINDER BLOCK AND CRANKSHAFT ARE REUSED

1.Measure cylinder block main bearing housing inner diameter and crankshaft main journal diameter. Refer to Inspection (GT-R certified NISSAN dealer).

2.Correspond the measured dimension in “Cylinder block main bearing housing inner diameter” row of “MAIN BEARING SELECTION TABLE”.

3.Correspond the measured dimension in “Crankshaft main journal diameter” column of “MAIN BEARING SELECTION TABLE”.

4.Follow step 3 and later in “When New Cylinder Block and Crankshaft are Used”.

MAIN BEARING SELECTION TABLE
MAIN BEARING GRADE TABLE (ALL JOURNALS)

Main bearing grade table (All journals) | : Refer to Main Bearing (GT-R certified NISSAN dealer).

UNDERSIZE BEARING USAGE GUIDE

- When the specified main bearing oil clearance is not obtained with standard size main bearings, use underside (US) bearing.
- When using undersize (US) bearing, measure the main bearing inner diameter with bearing installed, and grind main journal so that the main bearing oil clearance satisfies the standard.
  ■ CAUTION ■
  In grinding crankshaft main journal to use undersize bearings, keep the fillet R (A) [1.5 - 1.7 mm (0.059 - 0.067 in)].

Bearing undersize table | : Refer to Main Bearing (GT-R certified NISSAN dealer).