1.PREPARE BEFORE LEARNING With CONSULT-III

1. Turn the ignition switch ON.
2. Check the set values of “ADJUST CLUTCH A CAPACITY”, “ADJUST CLUTCH B CAPACITY”, “CLUTCH A TOUCH POINT”, and “CLUTCH B TOUCH POINT” in "Work support".
   ■ CAUTION ■
   Never erase each learning value and the clutch engagement pressure correction value.

Are the set values of all items 0?
YES>>GO TO 2.
NO>>Go to 2 after the set values become 0.
2.SET LEARNING CONDITION
With CONSULT-III

1. Start the engine.
2. Select “RANGE”, “ACCEL POSI SEN 1”, and “FLUID TEMP” in “Data Monitor”.
3. Set the condition as per the following.

   RANGE | : P
   ACCEL POSI SEN 1 | : 0.0/8
   FLUID TEMP | : 50 – 110 °C (122 – 230 °F)

Is the learning condition fulfilled?
YES>>GO TO 3.
NO>>Go to 3 after the learning condition is fulfilled.
3.PERFORM “CLUTCH GEAR LEARNING”
With CONSULT-III

1. Perform “CLUTCH GEAR LEARNING” in “Work support”.
2. Select “Start”.

■ CAUTION ■
The "CLUTCH GEAR LEARNING" must be completed at temperature within 50 – 110 °C (122 – 230 °F). The learning is not yet completed if the temperature condition is outside the specified value during learning.
Is "completed" displayed?
YES>>End of learning
NO>>GO TO 4.
4.CHECK THE LEARNING CONDITION
With CONSULT-III

1. Turn the ignition switch OFF, and wait for 15 seconds or more.
2. Start the engine.
3. Select “RANGE”, “ACCEL POSI SEN 1”, “FLUID TEMP”, “BATTERY VOLTAGE”, “ENGINE SPEED”, “VEHICLE SPEED”, and “LINE PRESSURE” in “Data Monitor”.
4. Check that the following learning condition is fulfilled.

   RANGE | : P
   ACCEL POSI SEN 1 | : 0.0/8
   FLUID TEMP | : 50 – 110 °C (122 – 230 °F)
   BATTERY VOLTAGE | : 11 V or more
   ENGINE SPEED | : 650 – 2,000 rpm
   VEHICLE SPEED | : 3.5 km/h (2 MPH) or less
   LINE PRESSURE | : 0.35 MPa (3.57 kg/cm2, 50.75 psi) or more

Is the learning condition fulfilled?
YES>>GO TO 5.
NO>>Go to 3 after the learning condition is fulfilled.
5.PERFORM “ACTIVE TEST” (CLUTCH A SOLENOID)
With CONSULT-III

1. Select “C/L A PRESS S/V” in “Active Test”.
2. Select “CLUTCH A PRESS”, and “TGT CLUTCH A PRS”.
3. Raise “CLUTCH A PRESS” to 1.0 MPa (10.2 kg/cm2, 145 psi), and then lower it to 0 MPa (0 kg/cm2, 0 psi).
4. Check that “CLUTCH A PRESS” and “TGT CLUTCH A PRS” follow with an equal value.

Do “CLUTCH A PRESS” and “TGT CLUTCH A PRS” follow with an equal value?
YES>>GO TO 6.
NO>>Check “Self Diagnostic Result” of “TRANSMISSION”.
6.PERFORM “ACTIVE TEST” (CLUTCH B SOLENOID)
With CONSULT-III

1. Select “C/L B PRESS S/V” in the “Active Test”.
2. Select “CLUTCH B PRESS”, and “TGT CLUTCH B PRS”.
3. Raise “CLUTCH B PRESS” to 1.0 MPa (10.2 kg/cm2, 145 psi), and then lower it to 0 MPa (0 kg/cm2, 0 psi).
4. Check that “CLUTCH B PRESS” and “TGT CLUTCH B PRS” follow with an equal value.

Do “CLUTCH B PRESS” and “TGT CLUTCH B PRS” follow with an equal value?
YES>>GO TO 3.
NO>>Check “Self Diagnostic Result” of “TRANSMISSION”.