NOTE： The details of time display are as follows.

- CRNT: A malfunction is detected now.
- PAST: A malfunction was detected in the past.

IGN counter is displayed on Freeze Frame Data. For details of Freeze Frame Data, refer to CONSULT-III Function (BCM - COMMON ITEM).

CONSULT display | Fail-safe | Freeze Frame Data

- Vehicle Speed
- Odo/Trip Meter
- Vehicle Condition

Intelligent Key warning lamp ON
Reference page
No DTC is detected. Further testing may be required. | — | — | — | —
U1000: CAN COMM | — | — | — | DTC Logic
U1010: CONTROL UNIT (CAN) | — | — | — | DTC Logic
U0415: VEHICLE SPEED SIG | — | — | — | DTC Logic
B2013: ID DISCORD BCM-S/L | × | × | — | DTC Logic
B2014: CHAIN OF S/L-BCM | × | × | — | DTC Logic
B2190: NATS ANTENNA AMP | × | — | — | DTC Logic
B2191: DIFFERENCE OF KEY | × | — | — | DTC Logic
B2192: ID DISCORD BCM-ECM | × | — | — | DTC Logic
B2193: CHAIN OF BCM-ECM | × | — | — | DTC Logic
B2195: ANTI SCANNING | × | — | — | DTC Logic
B2553: IGNITION RELAY | — | × | — | DTC Logic
B2555: STOP LAMP | — | × | — | DTC Logic
B2556: PUSH-BTN IGN SW | — | × | × | DTC Logic
B2557: VEHICLE SPEED | × | × | × | DTC Logic
B2560: STARTER CONT RELAY | × | × | × | DTC Logic
B2562: LOW VOLTAGE | — | × | — | DTC Logic
B2601: SHIFT POSITION | × | × | × | DTC Logic
B2602: SHIFT POSITION | × | × | × | DTC Logic
B2603: SHIFT POSI STATUS | × | × | × | DTC Logic
B2604: PNP SW | × | × | × | DTC Logic
B2605: PNP SW | × | × | × | DTC Logic
B2606: S/L RELAY | × | × | × | DTC Logic
B2607: S/L RELAY | × | × | × | DTC Logic
B2608: STARTER RELAY | × | × | × | DTC Logic
B2609: S/L STATUS | × | × | × | DTC Logic
B260A: IGNITION RELAY | × | × | × | DTC Logic
B260B: STEERING LOCK UNIT | — | × | × | DTC Logic
B260C: STEERING LOCK UNIT | — | × | × | DTC Logic
B260D: STEERING LOCK UNIT | — | × | × | DTC Logic
B260F: ENG STATE SIG LOST | × | × | × | DTC Logic
B2612: S/L STATUS | × | × | × | DTC Logic
B2614: ACC RELAY CIRC | — | × | × | DTC Logic
B2615: BLOWER RELAY CIRC | — | × | × | DTC Logic
B2616: IGN RELAY CIRC | — | × | × | DTC Logic
B2617: STARTER RELAY CIRC | × | × | × | DTC Logic
B2618: BCM | × | × | × | DTC Logic
B2619: BCM | × | × | × | DTC Logic
B261A: PUSH-BTN IGN SW | — | × | × | DTC Logic
B261E: VEHICLE TYPE | × | × | × (Turn ON for 15 seconds) | DTC Logic
B2621: INSIDE ANTENNA | — | × | — | DTC Logic
B2622: INSIDE ANTENNA | — | × | — | DTC Logic
B2623: INSIDE ANTENNA | — | × | — | DTC Logic
B26E7: TPMS CAN COMM | — | — | — | DTC Logic
B26E9: S/L STATUS | × | × | × (Turn ON for 15 seconds) | DTC Logic
B26EA: KEY REGISTRATION | — | × | × (Turn ON for 15 seconds) | DTC Logic