REMOVAL

1.Remove the door finisher. Refer to Removal and Installation.

2.Remove the inside handle cable from the inside handle. Remove the door lock knob cable from the door lock knob.
■ CAUTION ■
Never bend the cable end.

3.Remove the door window. Refer to Removal and Installation (GT-R certified NISSAN dealer).

4.Disengage the joint of key cylinder rod and outside handle rod at the outside handle side.

5.Remove the door lock assembly TORX bolts by the arrows in the figure.

6.Disconnect the door lock harness connector, and then remove the door lock assembly.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Apply anticorrosive agent onto the mounting surface.
- Check door lock cables are properly engaged with inside handle and outside handle.
- When installing key rod, rotate key rod holder until a click is felt.
- After installation, check door open/close, lock/unlock operation.