REMOVAL ■ CAUTION ■

- Before TCM is replaced, the IP characteristics must be extracted, based on the information read out from the malfunctioning TCM. For acquiring the IP characteristic data, refer to “CONSULT-III GT-R TCM CONFIGURATION MANUAL”.
- If no IP characteristic data can be extracted, TCM and the transmission assembly must be replaced as a set.

1.Disconnect battery cable from negative terminal.

2.Remove the trunk front finisher. Refer to Exploded View.

3.Disconnect the TCM harness connector with the following procedure.

- Push the protrusion for fixing and fully open the levers (A) as shown in the figure when disconnecting and connecting the TCM harness connector.

  1 | : TCM
  Direction B | : Disconnect
  Direction C | : Connect

4.Remove the TCM mounting bolt.

5.Remove the TCM from the vehicle.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■
Refer to Precautions for Replacement of TCM and Transmission Assembly (GT-R certified NISSAN dealer) when the TCM is replaced.