DESCRIPTION

- If the ignition switch is turned to the OFF position while the FRE switch is set to ON (manual FRE), “Perform the memory” or “Do not perform the memory” of FRE switch ON (manual FRE) condition can be selected.
- If “Perform the memory” was set, the FRE switch will be ON (manual FRE) when turning the ignition switch to the ON position again.
- If “Do not perform the memory” was set, the air inlets will be controlled automatically when turning the ignition switch to the ON position again.

HOW TO SET
With CONSULT-III
Perform the “FRE MEMORY SET” of HVAC work support item.

Work support items | Display | Setting
FRE MEMORY SET | WITHOUT | Perform the memory of manual FRE
WITH (initial status) | Do not perform the memory of manual FRE (auto control)

NOTE：
When the battery cable is disconnected from the negative terminal or when the battery voltage becomes 10 V or less, the setting of the FRE switch memory function may be cancelled.