1.CHECK GROUND CONNECTION

1. Turn A/C switch and blower fan switch OFF.
2. Turn ignition switch OFF.
3. Check ground connection M95. Refer to Ground Inspection in Circuit Inspection.

Is the inspection result normal?
YES>>GO TO 2.
NO>>Repair or replace ground connection.
2.CHECK REFRIGERANT PRESSURE SENSOR POWER SUPPLY CIRCUIT

1. Disconnect refrigerant pressure sensor harness connector.
2. Turn ignition switch ON.
3. Check the voltage between refrigerant pressure sensor harness connector and ground.

   Refrigerant pressure sensor | Ground | Voltage (V)
   Connector | Terminal
   E77 | 3 | Ground | Approx. 5

Is the inspection result normal?
YES>>GO TO 4.
NO>>GO TO 3.
3.DETECT MALFUNCTIONING PART
Check the following.

- Harness connectors M6, E106
- Harness connectors F103, M116
- Harness for open or short between ECM and refrigerant pressure sensor

>>Repair open circuit, short to ground or short to power in harness or connectors.
4.CHECK REFRIGERANT PRESSURE SENSOR GROUND CIRCUIT FOR OPEN AND SHORT

1. Turn ignition switch OFF.
2. Disconnect ECM harness connector.
3. Check the continuity between refrigerant pressure sensor harness connector and ECM harness connector.

   Refrigerant pressure sensor | ECM | Continuity
   Connector | Terminal | Connector | Terminal
   E77 | 1 | F102 | 74 | Existed

4. Also check harness for short to ground and short to power.

Is the inspection result normal?
YES>>GO TO 6.
NO>>GO TO 5.
5.DETECT MALFUNCTIONING PART
Check the following.

- Harness connectors M6, E106
- Harness connectors F103, M116
- Harness for open or short between ECM and refrigerant pressure sensor

>>Repair open circuit, short to ground or short to power in harness or connectors.
6.CHECK REFRIGERANT PRESSURE SENSOR INPUT SIGNAL CIRCUIT FOR OPEN AND SHORT

1. Check the continuity between refrigerant pressure sensor harness connector and ECM harness connector.

   Refrigerant pressure sensor | ECM | Continuity
   Connector | Terminal | Connector | Terminal
   E77 | 2 | F102 | 89 | Existed

2. Also check harness for short to ground and short to power.

Is the inspection result normal?
YES>>GO TO 8.
NO>>GO TO 7.
7.DETECT MALFUNCTIONING PART
Check the following.

- Harness connectors M6, E106
- Harness connectors F103, M116
- Harness for open or short between ECM and refrigerant pressure sensor

>>Repair open circuit, short to ground or short to power in harness or connectors.
8.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
Is the inspection result normal?
YES>>Replace refrigerant pressure sensor.
NO>>Repair or replace malfunctioning part.