1.CHECK COMBINATION METER OUTPUT SIGNAL

1. Connect CONSULT‐III.
2. Select the “DATA MONITOR” for the “METER/M&A”, then compare the “Fuel meter” monitor value with the fuel gauge reading on combination meter.

Fuel gauge indication position | Monitor value [L]
Full | Approx. 62.4
3/4 | Approx. 53.6
1/2 | Approx. 36.8
1/4 | Approx. 23.2
E | Approx. 11.2

Does the monitor value match the fuel gauge reading?
YES>>INSPECTION END
NO>>Replace the combination meter.