DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1754 | CONTROL UNIT (EEPROM) | Tire Pressure Monitoring System (TPMS) malfunction in the low tire pressure warning control unit occurs | Low tire pressure warning control unit malfunction

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Drive for several minutes at a speed of 40 km/h (25 MPH) or more, then stop the vehicle.
2. Stop the vehicle and perform self-diagnosis of the low tire pressure warning control unit.

Is DTC “C1754” detected?
YES>>Perform trouble diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END