DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1D02 | SIDE G-SENSOR SIG |

- A malfunction is detected in the side G sensor signal output from the yaw rate/side/decel G sensor to CAN communication.
- No transmission from the yaw rate/side/decel G sensor.

- Harness or connector (CAN communication line)
- ABS actuator and electric unit (control unit)
- E-SUS control unit

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Turn the ignition switch OFF to ON.
2. Perform “E-SUS” self-diagnosis.
3. Perform "ERASE MEMORY" in self-diagnosis.
4. Perform self-diagnosis of “E-SUS” again.

Is DTC “C1D02” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END