LOW TIRE PRESSURE WARNING LAMP SYMPTOM CHART

Diagnosis items | Symptom (Ignition switch ON) | Low tire pressure warning lamp | Cause | Action
Low tire pressure warning lamp | The low tire pressure warning lamp illuminates for 1 second, then turns OFF. |  | Wake-up operation for all transmitters at wheels is completed. | No system malfunctions
The low tire pressure warning lamp repeats blinking ON for 2 seconds and OFF for 0.2 seconds. |  | Wake-up operation for all transmitters at wheels is not completed. | Perform the wake-up operation for all transmitters at wheels. Refer to Transmitter Wake-up Procedure .
The low tire pressure warning lamp blinks once. |  | The front left transmitter is not activated. | Perform the wake-up operation for the transmitter at front left wheel. Refer to Transmitter Wake-up Procedure .
The low tire pressure warning lamp repeats blinking twice. |  | The front right transmitter is not activated. | Perform the wake-up operation for the transmitter at front right wheel. Refer to Transmitter Wake-up Procedure .
The low tire pressure warning lamp repeats blinking for 3 times. |  | The rear right transmitter is not activated. | Perform the wake-up operation for the transmitter at rear right wheel. Refer to Transmitter Wake-up Procedure .
The low tire pressure warning lamp repeats blinking for 4 times. |  | The rear left transmitter is not activated. | Perform the wake-up operation for the transmitter at rear left wheel. Refer to Transmitter Wake-up Procedure .
The low tire pressure warning lamp turns ON and stays illuminated. |  | Low tire pressure | Check with CONSULT-III the tire pressure values. Refer to CONSULT-III Function (GT-R certified NISSAN dealer).
Low tire pressure warning lamp | The low tire pressure warning lamp repeats blinking at 0.5-second intervals for 1 minute, and then stays illuminated. |  | The combination meter fuse is open or removed (or pulled out). | Check and install the combination meter fuse. If necessary, replace the fuse.
The low tire pressure warning control unit harness connector is removed. | Check the connection conditions of the low tire pressure warning control unit harness connector, and repair if necessary.
Tire Pressure Monitoring System (TPMS) malfunction. |

- Perform CONSULT-III self-diagnosis. Refer to CONSULT-III Function (GT-R certified NISSAN dealer).
- If necessary, perform transmitter ID registration. Refer to Transmitter ID Registration Procedure.

Turn signal lamp | The turn signal lamps do not blink twice when the transmitter is activated. Or the buzzer does not sound. | — |

1. The transmitter activation tool (J-45295) does not activate.
2. The ignition switch is OFF when the transmitter wake-up operation is performed.
3. The transmitter activation tool (J-45295) is not used in the correct position.
4. The transmitter is already waked up.

1. Replace the battery in the transmitter activation tool (J-45295).
2. Turn the ignition switch ON when performing the transmitter wake-up operation.
3. Operate the transmitter activation tool (J-45295) in the correct position when performing the wake-up operation.
4. No procedure.

NOTE：
If transmitter wake-up operation is not completed for two or more transmitters, the applicable low tire pressure warning lamp blinking patterns are displayed continuously.
(Example: Blinks once/OFF/blinks 3 times = Wake-up operation is not completed at the front left wheel and rear right wheel transmitters.)