1.STEERING ANGLE SENSOR ADJUSTMENT, DECEL G SENSOR CALIBRATION, PRESSURE SENSOR CALIBRATION, AND VALVE CALIBRATION After replacing an ABS actuator and electric unit (control unit), be sure to perform the following procedure.

- Steering angle sensor adjustment: Refer to Description (GT-R certified NISSAN dealer).
- Decel G sensor calibration: Refer to Description (GT-R certified NISSAN dealer).
- Pressure sensor calibration: Refer to Description (GT-R certified NISSAN dealer).
- Valve calibration: Refer to Description (GT-R certified NISSAN dealer).

>>END