REMOVAL

1.Remove engine undercover. Refer to Exploded View.

2.Remove front undercover. Refer to Exploded View.

3.Drain engine coolant from radiator drain plug at the bottom of radiator. Refer to Draining.
■ CAUTION ■

- Perform this step when the engine is cold.
- Never spill engine coolant on drive belt.

4.Remove air duct and air cleaner case assembly (LH). Refer to Exploded View.

5.Remove reservoir tank. Refer to Exploded View (GT-R certified NISSAN dealer).

6.Disconnect radiator hose (lower) and water hose at water inlet and thermostat assembly side.

7.Disconnect intake valve timing control solenoid valve harness connector (bank 2).

8.Remove water inlet and thermostat assembly (1).

A | : Never loosen these screws.

■ CAUTION ■
Never disassemble water inlet and thermostat assembly. Replace them as a unit, if necessary.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Replace water hose clamp if it is removed.
- Be careful not to spill engine coolant over engine room. Use rag to absorb engine coolant.