1.UNIT INSPECTION OF METER CONTROL SWITCH

1. Turn the ignition switch OFF.
2. Disconnect the meter control switch connector.
3. Check the continuity of meter control switch.

   Terminal No. | Operation and status | Continuity
   6 | 2 | Press the enter switch | Existed
   Other than the above | Not existed
   7 | 2 | Press the select switch | Existed
   Other than the above | Not existed
   8 | 2 | Press the trip A/B reset switch. | Existed
   Other than the above | Not existed
   3 | 2 | Press the switch | Existed
   Other than the above | Not existed
   1 | 2 | Press the switch | Existed
   Other than the above | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the meter control switch.