DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
U1000 | CAN COMM CIRCUIT | E-SUS control unit does not communicates the CAN communication signal for 2 seconds or more. | CAN communication malfunction

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Turn the ignition switch OFF to ON.
2. Perform “E-SUS” self-diagnosis.

Is DTC “U1000” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END