When the combination meter receives the signal of the malfunction via CAN communication from the low tire pressure warning control unit, it displays a message on the information display and warns the driver of the tire pressure and the Tire Pressure Monitoring System (TPMS) status.

Condition | Information display
Ignition switch OFF. | Nothing displayed.
Tire pressure is low. Tire pressure is 150 kPa (1.5 kg/cm2, 22 psi) or less |
Tire is flat. Tire pressure is 70 kPa (0.7 kg/cm2, 10 psi) or less |
Tire Pressure Monitoring System (TPMS) malfunction |