1.CHECK DTC Check that DTC UXXXX, P0500 or P1574 is not displayed. Is the inspection result normal? YES>>GO TO 2. NO-1>>Perform trouble diagnosis for DTC UXXXX.
NO-2>>Perform trouble diagnosis for DTC P0500. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO-3>>Perform trouble diagnosis for DTC P1574. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
2.CHECK DTC WITH “COMBINATION METER”
Refer to CONSULT-III Function (METER/M&A).
Is the inspection result normal?
YES>>GO TO 3.
NO>>Perform trouble diagnosis relevant to DTC indicated.
3.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
Is the inspection result normal?
YES>>Replace combination meter.
NO>>Repair or replace.