1.CHECK OIL PRESSURE SENSOR CIRCUIT

1. Turn the ignition switch OFF.
2. Disconnect the connectors of combination meter and oil pressure sensor.
3. Check for continuity between the combination meter harness connector and the oil pressure sensor harness connector.

   Combination meter | Oil pressure sensor | Continuity
   Connector | Terminal | Connector | Terminal
   M53 | 34 | E255 | 1 | Existed
   M53 | 35 | E255 | 2 | Existed
   M53 | 14 | E255 | 3 | Existed

4. Check for continuity between the combination meter harness connector and the ground.

   Combination meter | Ground | Continuity
   Connector | Terminal
   M53 | 34 | Not existed
   M53 | 35 | Not existed
   M53 | 14 | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Repair the harnesses or connectors.