REMOVAL Driver Side

1.Set the temperature (driver side) at 18.0°C (60°F).

2.Disconnect the battery cable from the negative terminal.
■ CAUTION ■
The angle may be out, when installing the air mix door motor to the air mix door, unless the above 2 procedures are performed.

3.Remove instrument lower panel (driver). Refer to Exploded View.

4.Remove mounting screws of air mix door motor, and then remove air mix door motor.

5.Disconnect air mix door motor connector.

Passenger Side

1.Set the temperature (passenger side) at 18.0°C (60°F).

2.Disconnect the battery cable from the negative terminal.
■ CAUTION ■
The angle may be out, when installing the air mix door motor to the air mix door, unless the above 2 procedures are performed.

3.Remove instrument lower panel (assist). Refer to Exploded View.

4.Remove mounting screws of air mix door motor, and then remove air mix door motor.

5.Disconnect air mix door motor connector.

INSTALLATION
Installation is basically the reverse order of removal.