1.CHECK ELECTRIC THROTTLE CONTROL ACTUATOR VISUALLY

1. Turn ignition switch OFF.
2. Remove the intake air duct.
3. Check if foreign matter is caught between the throttle valve (1) and the housing.

Is the inspection result normal?
YES>>GO TO 2.
NO>>Remove the foreign matter and clean the electric throttle control actuator inside.
2.REPLACE ELECTRIC THROTTLE CONTROL ACTUATOR

1. Replace malfunctioning electric throttle control actuator.
2. Go to Special Repair Requirement (GT-R certified NISSAN dealer).

>>INSPECTION END