REMOVAL

1. Remove the instrument lower panel (driver). Refer to Exploded View.
2. Remove instrument pad B. Refer to Exploded View.
3. Remove the mounting screw for the low tire pressure warning control unit.
4. Disconnect the low tire pressure warning control unit harness connector.
5. Remove the low tire pressure warning control unit.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Perform ID registration after replacing low tire pressure warning control unit. Refer to Transmitter ID Registration Procedure.