BRAKE FLUID LEVEL

- Check that the fluid level in the reservoir tank is within the specified range (MAX – MIN lines).
- Visually check for any brake fluid leakage around the reservoir tank.
- Check the brake system for any leakage if the fluid level is extremely low (lower than MIN).
- Check the brake system for fluid leakage if the warning lamp remains illuminated even after the parking brake lever is released.

BRAKE LINE

1.Check the brake line (tube and hose) for any cracks or damage.
■ CAUTION ■
Replace with new ones if necessary.

2.Depress the brake pedal with a force of 785 N (80 kg, 176 lb) and hold down the pedal for approximately 5 seconds with the engine running. Check for any fluid leakage.
■ CAUTION ■
Retighten each part to the specified torque and repair any abnormal (damaged, worn, or deformed) part if any fluid leakage is present.