1.CHECK HEADLAMP (LO) OPERATION IPDM E/R AUTO ACTIVE TEST

1. Activate IPDM E/R auto active test. Refer to Diagnosis Description.
2. Check that the headlamp (LO) is turned ON.

CONSULT-III ACTIVE TEST

1. Select “EXTERNAL LAMPS” of IPDM E/R active test item.
2. With operating the test items, check that the headlamp (LO) is turned ON.

   Lo | : Headlamp (LO) ON
   Off | : Headlamp (LO) OFF

Is the headlamp (LO) turned ON/OFF?
YES>>Headlamp (LO) is normal.
NO>>Refer to Diagnosis Procedure.