- The combination meter receives the engine speed signal from ECM and the shift position signal (manual mode range) from TCM via CAN communication, and illuminates/turns off/blinks the up-shift indicator.
- The engine speed at which the up-shift indicator is illuminated/turned off/blinked can be set with the setting function of information display.

- OFF: All of the up-shift indicators do not illuminate.
- 3,000 to 6,300 rpm: Engine speed can be set at which the up-shift indicator (green) is illuminated.
- AUTO: Up-shift indicator (green) does not illuminate. The up-shift indicator (yellow) and up-shift indicator (red) is turned on/off according to the set value.

UP-SHIFT INDICATOR (GREEN)

- Using the setting function of information display, the up-shift warning speed can be set.
- The up-shift indicator (green) is illuminated/turned off/blinked according to the engine speed.

- OFF: If the actual engine speed is lower than the arbitrarily set engine speed, which is 3,000 to 6,300 rpm set by the setting function of information display, by 500 rpm or more, the up-shift warning lamp is turned OFF. Also, while the up-shift indicator (green) is blinking or illuminated, if the actual engine speed becomes lower than the arbitrarily set engine speed by 600 rpm or more, the up-shift warning lamp is turned OFF.
- Blink: If the actual engine speed is lower than the arbitrarily set engine speed by 500 rpm or more, the up-shift indicator (green) is blinked.
- ON: When the actual engine speed exceeds the arbitrarily set engine speed, the up-shift indicator (green) is illuminated.Also, while the up-shift indicator (green) is blinking or illuminated, if the actual engine speed becomes lower than the arbitrarily set engine speed by 100 rpm or more, the up-shift indicator is blinked.

UP-SHIFT INDICATOR (YELLOW)
The up-shift indicator (yellow) is turned ON/OFF according to the engine speed.

- OFF: When the engine speed is less than 6,300 rpm, the up-shift indicator (yellow) does not illuminate.Also, while the up-shift indicator (yellow) is illuminated, when the engine speed becomes 6,200 rpm or lower, the up-shift indicator (yellow) is turned OFF.
- ON: When the engine speed becomes 6,300 rpm or more, the up-shift indicator (yellow) is illuminated.

UP-SHIFT INDICATOR (RED)
The up-shift indicator (red) is turned ON/OFF according to the engine speed.

- OFF: When the engine speed is less than 6,800 rpm, the up-shift indicator (red) does not illuminate.Also, while the up-shift indicator (red) is illuminated, when the engine speed becomes 6,700 rpm or lower, the up-shift indicator (red) is turned OFF.
- ON: When the engine speed becomes 6,800 rpm or more, the up-shift indicator (red) is illuminated.