Type | A002TX0091
MITSUBISHI make
Nominal rating | [V - A] | 12 ‐150
Ground polarity |  | Negative
Minimum revolution under no-load (When 13.5 V is applied) | [rpm] | Less than 1,300
Hot output current (When 13.5 V is applied) | [A/rpm] | More than 57/1,500 More than 126/2,500 More than 152/5,000
Regulated output voltage | [V] | 14.1 - 14.7
Minimum length of brush | [mm (in)] | More than 5.00 (0.197)
Brush spring pressure | [N (g, oz)] | 4.1 - 5.3 (418 - 541, 14.7 - 19.1)
Slip ring minimum outer diameter | [mm (in)] | More than 22.1 (0.870)
Rotor (Field coil) resistance | [Ω] | 1.8 - 2.2