REMOVAL

1.Remove tires with power tool. Refer to Exploded View.

2.Remove rear diffuser. Refer to Exploded View.

3.Remove main muffler assembly. Refer to Exploded View.

4.Remove cap, and then stabilizer connecting rod.
■ CAUTION ■
Apply a matching mark to identity the installation position.

5.Remove stabilizer connecting rod mounting bracket.

6.Remove stabilizer clamp and stabilizer bushing, and then remove stabilizer bar.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Check the matching mark when installing.
- Tighten the mounting nut to the specified torque while holding a hexagonal part of stabilizer connecting rod side.