REMOVAL

1.Remove the front seat. Refer to Removal and Installation.

2.Remove the seat cushion outer finisher (1). Refer to Disassembly and Assembly.

3.Remove the screws (A).

4.Remove the heater seat switch (2) from the seat cushion outer finisher.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- When performing the work, use shop cloths to protect the parts from damage.
- Always fix the harness clamp in the normal position.