REMOVAL Dovetail Male

1.Remove the door inner west reinforcement. Refer to Exploded View.

2.Fix the nut in the door panel using tools, and then rotate the dovetail male to remove.
■ CAUTION ■
Never drop the nuts in the door panel.

Dovetail Female

1.Remove the dovetail female cover.

2.Remove the rear side finisher. Refer to Exploded View.

3.Remove the mounting bolts, and then remove the dovetail female.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Be careful about the direction of the dovetail male mounting nut.
- Check the engagement between dovetail female and dovetail male for noise or looseness when closing the door.