REMOVAL

1.Remove engine cover with power tool. Refer to Exploded View.

2.Remove intake manifold collector. Refer to Exploded View.
■ CAUTION ■
Mark the parts with paint in advance of the reinstallation to prevent misalignment between the intake manifold collector and intake manifold.

3.Remove ignition coil.

4.Remove spark plug with a spark plug wrench (commercial service tool).

a | : 14 mm (0.55 in)

■ CAUTION ■
Never drop or shock spark plug.

INSTALLATION
Installation is the reverse order of removal.