DTC DETECTION LOGIC

DTC | Self-diagnosis item | DTC detection condition | Possible cause
P0747 | Pressure sontrol solenoid "A" stuck on | A DTC is set if the clutch A pressure sensor value is higher than the clutch A pressure target value by 0.2 MPa (2.04 kg/cm2, 29 psi) or more. |

- Clutch A solenoid valve
- Clutch A pressure sensor
- Clutch A oil passage
- Harness or connector
  (Open or short in the clutch A solenoid valve circuit)
  (Open or short in the clutch A pressure sensor circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Turn the ignition switch ON.
2. Shift the shift lever to the N position.
3. Start the engine.
4. Select “RANGE” and “GEAR” in “Data Monitor”.
5. With the vehicle stationary, maintain the following conditions for 5 seconds or more.

   RANGE | : M
   GEAR | : 2

6. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Turn the ignition switch ON.
2. Shift the shift lever to the N position.
3. Start the engine.
4. With the vehicle stationary, maintain the following conditions for 5 seconds or more.

   Shift lever | : M range
   Gear | : 2

5. Check self-diagnosis.

Is DTC P0747 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.