DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P1705 | Throttle position CAN signal compatibility | A DTC is set if TCM detects a difference between 2 signals of the throttle position (CAN signal). |

- Accelerator pedal position sensor
- ECM
- Harness or connector
  (Open or short in the accelerator pedal position sensor signal circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine and run at idle for 5 seconds or more.
2. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine and run at idle for 5 seconds or more.
2. Check self-diagnosis.

Is DTC P1705 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.