REMOVAL

1.Remove the front seat. Refer to Removal and Installation.

2.Disconnect the thigh support switch connector.

3.Remove the seat cushion outer finisher (1). Refer to Disassembly and Assembly.

4.Remove the thigh support switch (2) from the seat cushion outer finisher (1) while pressing the pawls.

| : Pawl

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- When performing the work, use shop cloths to protect the parts from damage.
- Always fix the harness clamp in the normal position.